Testcases for Device Access Credentials:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Testcase Number** | **Description** | **Test data** | **Expected Output** | **Actual Output** | **Result** |
| Testcase 01 | API call to check active or not. | IP:port/device/active | Response: ACTIVE | Response: ACTIVE | Passed |
| Testcase 02 | API call to update credentials. | IP:port /device/setpubcred  Payload:  Public Access Username- OXZYNMCPKELTLS  Public Access Password: HNJ3EZ=)INNOX++TGK  Private Access Username- JOPEKZQPDI  Private Access Password: FKWPC#MO#YXWKBLL | Update the PubAC file in device.  Response: SUCCESS | PubAC and PvtAC files updated  Response: SUCCESS | Passed |
| Testcase 03 | API call to use credentials PubAC through Public IP and device switch STATE = CMan | IP:port/access  Payload:  Public Access Username- OXZYNMCPKELTLS  Public Access Password: HNJ3EZ=)INNOX++TGK | Response: ACCESS | Response: ACCESS | Passed |
| Testcase 04 | API call to use credentials PubAC through Public IP and device switch STATE = LMan | IP:port/access  Payload:  Public Access Username- OXZYNMCPKELTLS  Public Access Password: HNJ3EZ=)INNOX++TGK | Response: Access not allowed!!! | Response: Access not allowed!!! | Passed |
| Testcase 05 | API call to use credentials PvtAC through Public IP and device switch STATE = LMan | IP:port/access  Payload:  Private Access Username- JOPEKZQPDI  Private Access Password: FKWPC#MO#YXWKBLL | Response: Access not allowed!!! | Response: Access not allowed!!! | Passed |
| Testcase 06 | API call to use credentials PvtAC through Private IP and device switch STATE = LMan | IP:port/access  Payload:  Private Access Username- JOPEKZQPDI  Private Access Password: FKWPC#MO#YXWKBLL | Response: ACCESS | Response: ACCESS | Passed |